SIMISA@@@@@@@@@@JINX0h0t______

Tr_CabViewFile (
	CabViewType ( 1 )
	CabViewFile ( ETR450front1024.ace )
	CabViewWindow ( 0 0 640 480 )
	CabViewWindowFile ( ETR450front1024.ace )
	Position ( -1.5 3.5 6 )
	Direction ( 10 0 0 )
	CabViewFile ( ETR450left1024.ace )
	CabViewWindow ( 0 0 640 480 )
	CabViewWindowFile ( ETR450left1024.ace )
	Position ( -0.5 2.5 7 )
	Direction ( 5 -65 0 )
	CabViewFile ( ETR450right1024.ace )
	CabViewWindow ( 0 0 640 480 )
	CabViewWindowFile ( ETR450right1024.ace )
	Position ( 0.5 2.5 7 )
	Direction ( 5 65 0 )
	EngineData ( ETR450 )
	CabViewControls ( 23
		Dial (
			Type ( SPEEDOMETER DIAL )
			Position ( 338 216 15 30 )
			Graphic ( whiteneedle_m.ace )
			Style ( NEEDLE )
			ScaleRange ( 0 320 )
			ScalePos ( 200 160 )
			Units ( KM_PER_HOUR )
			Pivot ( 23 )
			DirIncrease ( 0 )
		)
		Dial (
			Type ( MAIN_RES DIAL )
			Position ( 169 220 15 15 )
			Graphic ( redneedle_sss.ace )
			Style ( NEEDLE )
			ScaleRange ( 0 160 )
			ScalePos ( 214 145 )
			Units ( PSI )
			Pivot ( 12 )
			DirIncrease ( 0 )
		)
		Dial (
			Type ( EQ_RES DIAL )
			Position ( 169 219 15 15 )
			Graphic ( whiteneedle_sss.ace )
			Style ( NEEDLE )
			ScaleRange ( 0 160 )
			ScalePos ( 214 145 )
			Units ( PSI )
			Pivot ( 12 )
			DirIncrease ( 0 )
		)
		Dial (
			Type ( BRAKE_CYL DIAL )
			Position ( 171 257 15 15 )
			Graphic ( whiteneedle_sss.ace )
			Style ( NEEDLE )
			ScaleRange ( 0 160 )
			ScalePos ( 214 145 )
			Units ( PSI )
			Pivot ( 12 )
			DirIncrease ( 0 )
		)
		Dial (
			Type ( BRAKE_PIPE DIAL )
			Position ( 135 258 15 15 )
			Graphic ( whiteneedle_sss.ace )
			Style ( NEEDLE )
			ScaleRange ( 0 160 )
			ScalePos ( 214 145 )
			Units ( PSI )
			Pivot ( 12 )
			DirIncrease ( 0 )
		)
		TwoState (
			Type ( SANDERS TWO_STATE )
			Position ( 318 328 33 23 )
			Graphic ( ETR450sand.ace )
			NumFrames ( 2 2 1 )
			Style ( ONOFF )
			MouseControl ( 1 )
		)
		TwoState (
			Type ( PANTOGRAPH TWO_STATE )
			Position ( 117 289 11 11 )
			Graphic ( ETR450slideSW.ace )
			NumFrames ( 2 2 1 )
			Style ( ONOFF )
			MouseControl ( 1 )
		)
		TriState (
			Type ( DIRECTION TRI_STATE )
			Position ( 169 308 30 41 )
			Graphic ( ETR450reverser.ace )
			NumFrames ( 3 3 1 )
			Style ( NONE )
			MouseControl ( 1 )
			Orientation ( 1 )
			DirIncrease ( 1 )
		)
		TwoState (
			Type ( HORN TWO_STATE )
			Position ( 607 296 25 51 )
			Graphic ( ETR450horn.ace )
			NumFrames ( 2 2 1 )
			Style ( WHILE_PRESSED )
			MouseControl ( 1 )
		)
		Lever (
			Type ( TRAIN_BRAKE LEVER )
			Position ( 210 293 55 67 )
			Graphic ( ETR450t_brake.ace )
			Style ( NOT_SPRUNG )
			MouseControl ( 1 )
			NumFrames ( 12 4 3 )
			NumPositions ( 0 )
			NumValues ( 0 )
			Orientation ( 1 )
			DirIncrease ( 1 )
			ScaleRange ( 0 1 )
		)
		Lever (
			Type ( THROTTLE LEVER )
			Position ( 393 313 33 80 )
			Graphic ( ETR450throttle.ace )
			Style ( NOT_SPRUNG )
			MouseControl ( 1 )
			NumFrames ( 12 4 3 )
			NumPositions ( 0 )
			NumValues ( 0 )
			Orientation ( 1 )
			DirIncrease ( 1 )
			ScaleRange ( 0 1 )
		)
		CabSignalDisplay (
			Type ( ASPECT_DISPLAY CAB_SIGNAL_DISPLAY )
			Position ( 324 312 46 12 )
			Graphic ( ETR450cabsegnali.ace )
		)
		TriState (
			Type ( FRONT_HLIGHT TRI_STATE )
			Position ( 171 289 11 11 )
			Graphic ( ETR450slideSW.ace )
			NumFrames ( 2 2 1 )
			Style ( NONE )
			MouseControl ( 1 )
			Orientation ( 1 )
			DirIncrease ( 1 )
		)
		TwoState (
			Type ( RESET TWO_STATE )
			Position ( 282 383 24 20 )
			Graphic ( ETR450reset.ace )
			NumFrames ( 2 2 1 )
			Style ( ONOFF )
			MouseControl ( 1 )
		)
		TwoState (
			Type ( EMERGENCY_BRAKE TWO_STATE )
			Position ( 3 367 32 32 )
			NumFrames ( 0 0 0 )
			Style ( ONOFF )
			MouseControl ( 1 )
		)
		Gauge (
			Type ( LOAD_METER GAUGE )
			Position ( 260 223 7 20 )
			Area ( 0 0 10 10 )
			Graphic ( ETR450pointer_y.ace )
			Style ( POINTER )
			ScaleRange ( 0 2000 )
			ZeroPos ( 0 )
			PositiveColour ( 1
				ControlColour ( 0 0 0 )
			)
			NegativeColour ( 0 )
			Orientation ( 1 )
			DirIncrease ( 1 )
			Units ( AMPS )
		)
		Gauge (
			Type ( LOAD_METER GAUGE )
			Position ( 278 222 7 20 )
			Area ( 0 0 10 10 )
			Graphic ( ETR450pointer_y.ace )
			Style ( POINTER )
			ScaleRange ( 0 2000 )
			ZeroPos ( 0 )
			PositiveColour ( 1
				ControlColour ( 0 0 0 )
			)
			NegativeColour ( 0 )
			Orientation ( 1 )
			DirIncrease ( 1 )
			Units ( AMPS )
		)
		TwoState (
			Type ( PANTOGRAPH TWO_STATE )
			Position ( 130 289 11 11 )
			Graphic ( ETR450slideSW.ace )
			NumFrames ( 2 2 1 )
			Style ( ONOFF )
			MouseControl ( 1 )
		)
		Gauge (
			Type ( LINE_VOLTAGE GAUGE )
			Position ( 239 222 7 20 )
			Area ( 0 0 10 10 )
			Graphic ( ETR450pointer_y.ace )
			Style ( POINTER )
			ScaleRange ( 0 30000 )
			ZeroPos ( 0 )
			PositiveColour ( 1
				ControlColour ( 0 0 0 )
			)
			NegativeColour ( 0 )
			Orientation ( 1 )
			DirIncrease ( 1 )
			Units ( VOLTS )
		)
		MultiStateDisplay (
			Type ( OVERSPEED MULTI_STATE_DISPLAY )
			Position ( 349 274 14 5 )
			Graphic ( ETR450redON.ace )
			States ( 2 2 1
				State (
					Style ( 0 )
					SwitchVal ( 0 )
				)
				State (
					Style ( 0 )
					SwitchVal ( 1 )
				)
			)
		)
		MultiStateDisplay (
			Type ( WHEELSLIP MULTI_STATE_DISPLAY )
			Position ( 295 259 14 5 )
			Graphic ( ETR450redON.ace )
			States ( 2 2 1
				State (
					Style ( 0 )
					SwitchVal ( 0 )
				)
				State (
					Style ( 0 )
					SwitchVal ( 1 )
				)
			)
		)
		MultiStateDisplay (
			Type ( FRICTION_BRAKING MULTI_STATE_DISPLAY )
			Position ( 279 259 14 5 )
			Graphic ( ETR450redON.ace )
			States ( 2 2 1
				State (
					Style ( 0 )
					SwitchVal ( 0 )
				)
				State (
					Style ( 0 )
					SwitchVal ( 1 )
				)
			)
		)
		MultiStateDisplay (
			Type ( PANTO_DISPLAY MULTI_STATE_DISPLAY )
			Position ( 263 259 14 5 )
			Graphic ( ETR450redON.ace )
			States ( 2 2 1
				State (
					Style ( 0 )
					SwitchVal ( 0 )
				)
				State (
					Style ( 0 )
					SwitchVal ( 1 )
				)
			)
		)
	)
)