For english see below

Carrozza di 2° classe per medie distanze
Serie npBD (vestiboli centrali semipilota non passante)

50 83 82 79 301

Carrozza della prima serie - dalla 79 300 alla 79 303 - atta esclusivamente al telecomando 
con locomotori della serie D445 (identificabili dalla scritta TD sotto il fianco della 
cabina), mentre la seconda serie - dalla 79 304 alla 79 378 - (almeno per le prime 19 
vetture) differiva per la porta scorrevole del bagagliaio postaall'esterno delle fiancate. 
Viene ancora oggi usata per treni Regionali ed  Interregionali, quasi tutte ricolorate nella livrea XMPR.


Modello originale di Mr.Rokko con cabina della D345 messa a disposizione da Vittorio dell'Aquila
Repaint di Ernesto Imperato


Per l'installazione basta scompattare il file e copiare la cartella 'FS_npBD_TD
nella directory TRAINS/TRAINSET di TS, per creare poi il proprio consist.


(c) by Ernesto Imperato, emsa@libero.it (per qualsiasi domanda)


Passenger car npBD 50 83 82 79 301 by FS Ferrovie dello Stato (Italy)

Carriage build in '80 for use exlusive with Diesel Engine D445.
Used for regional and interregional train, today in XMPR scheme.

Unzip the file into TRAINSET folder of TS. Made a new consists.

Original 3D model by Mr.Rokko. Cab by Vittorio dell'Aquila.
Repaint by Ernesto Imperato (emsa@libero.it)


