----------------------------------------------
Italian steam engine Gr. 835
Version 1.0 of 20 July 2005
----------------------------------------------

Shunting steam engines.

		
Max speed: 55 km/h	
Boiler pressure: 12 kg/cm²	
Total Weight: 45.3 t	
Adeasion Weight: 45.3 t		
Quantity: 370			
Build in: 1906-22

Pack content:

Steam engine Gr. 83701   used in between 1911-1920
Steam engine Gr. 835.212 used in between 1920-1964
Steam engine Gr. 740.034 used in between 1950-1978


Installation:
1. Unzip all in main Train Simulator folder, checking if Winzip has checked
"Use folder    names" box.
2. Use the editor to make a consist.



- Repainter notice: this model can be freely repainted, but the repainted version
MUST give credit to the authors of this work, it can not be sold, and the author of
the repaint must tell me of his work and of a site to download it.

- This model is freeware.
This means it can be redistributed, but only if not modified: no files can be deleted
from this archive, and no files can be added to the archive without the author
authorization. This file can not be sold on the internet, or via optical or magnetic
storage devices, or in any other way: you can't make money from this file. The author
can ask sites publishing this file, to remove it. "Theft" of this material
(all the files in this archive) will not be tolerated.

Renzo Grassi, rgrassi@df.unipi.it