----------------------------------------------
Italian steam engine Gr. 740, Gr.743 and Gr.741
Version 3.0 of August 2007
----------------------------------------------

The steam engines Gr. 740 were made improving the project of Gr. 730 
modifying boiler and trasmission system (with superheated steam).
For the success of this engine, 470 units were built, in 1911-23.
These engines were used as freight trains in rail roads with average traffic.
The Gr.743 and Gr.741 are the powerful version on Gr.740

Max speed: 65 km/h
Power: 980 CV (749), 1100 (743-741) a 45 km/h
Boiler pressure: 12 kg/cm²
Quantity 470 (740), 94 (743), 81 (741)
Construction period 1911-23 (740), 1941, 1951-54 (743), 1954, 1958-60 (741)

Pack content:

Steam Engine Gr. 74122		setting on 1911 to 1920
Steam Engine Gr. 740.084	setting on 1918 to 1950
Steam Engine Gr. 740.316	setting on 1950 to 1974
Steam Engine Gr. 741.142	setting on 1954 to 1974
Steam Engine Gr. 743.073	setting on 1951 to 1974 with snowplough
Steam Engine Gr. 743.410	setting on 1951 to 1974


Installation:
1. Unzip all in main Train Simulator folder, checking if Winzip has checked
"Use folder    names" box.
2. Use the editor to make a consist.



- Repainter notice: this model can be freely repainted, but the repainted version
MUST give credit to the authors of this work, it can not be sold, and the author of
the repaint must tell me of his work and of a site to download it.

- This model is freeware.
This means it can be redistributed, but only if not modified: no files can be deleted
from this archive, and no files can be added to the archive without the author
authorization. This file can not be sold on the internet, or via optical or magnetic
storage devices, or in any other way: you can't make money from this file. The author
can ask sites publishing this file, to remove it. "Theft" of this material
(all the files in this archive) will not be tolerated.

Renzo Grassi, rgrassi@df.unipi.it