SIMISA@@@@@@@@@@JINX0D0t______

Wagon ( FS_GR740_084  
	Type ( Engine )
	WagonShape ( FS_GR740_084.s )
	Size  ( 2.7m 4.12m 10.9m )
	CentreOfGravity ( 0m 1.86m 0m )
	Centre ( 0m 0m 0m )
	Mass ( 66.5t )
	InertiaTensor ( Box(2.7m 4.0m 10.9m) )
	Coupling (
		Type ( chain )
		Spring (
			Stiffness ( 1e1N/m 1e6N/m )
			Damping ( 1e7N/m 1e7N/m)
			Break ( 3.2e6N 3.2e6N )
			r0 ( 0m 0.078m )
		)
	)
	
	Adheasion ( 0.15 0.3 2 0.5 )
	DerailRailHeight ( 4cm )
	DerailRailForce ( 240kN )
	DerailBufferForce ( 400kN )
	WheelRadius ( 0.43m)
	NumWheels ( 1 )
	Friction (
		50N/m/s			1		-1mph		0		1
		5.1N/rad/s		1		-1rad/s		0		1
	)

	BrakeEquipmentType( "Triple_valve, Auxilary_reservoir, Handbrake" )
	BrakeSystemType( "Air_single_pipe" )
	MaxBrakeForce( 66kN )

	MaxHandbrakeForce( 60kN )
	NumberOfHandbrakeLeverSteps( 100 )

	TripleValveRatio( 2.5 )
	MaxReleaseRate( 15 )
	MaxApplicationRate( 15 )
	MaxAuxilaryChargingRate( 15 )
        BrakeCylinderPressureForMaxBrakeBrakeForce( 70 )

	Lights	( 5
		Light	(
			comment( Sphere of light )
			Type( 1 )
			Conditions(
				Headlight ( 3 )
				Unit ( 2 )
				)
			Cycle	( 0 )
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			States	( 1
				State	(
					Duration ( 0.0 )
					LightColour ( ffffffd5 )
					Position ( 0.0 10 0 )
					Transition ( 0 )
					Radius ( 160.0 )
					Angle ( 25.0 )
					)
				)
			)
			
		
		Light	(	
			comment( Head light right dim )
			Type( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 2 )
				)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle	( 0 )
			States	( 1
				State	(
					Duration ( 0.0 )
					LightColour ( cdffffd5 )
					Position ( -0.87 1.645 4.95 )
					Azimuth ( 0.0 0.0 5.0 )
					Transition ( 0 )
					Radius ( 0.5 )
					)
				)
			)
		Light	(	
			comment( Head light right dim )
			Type( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 2 )
				)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle	( 0 )
			States	( 1
				State	(
					Duration ( 0.0 )
					LightColour ( cdffffd5 )
					Position ( -0.87 1.716 4.95 )
					Azimuth ( 0.0 0.0 5.0 )
					Transition ( 0 )
					Radius ( 0.5 )
					)
				)
			)

		Light	(
			comment( Head light left dim )
			Type( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 2 )
				)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle	( 0 )
			States	( 1
				State	(
					Duration ( 0.0 )
					LightColour ( cdffffd5 )
					Position ( 0.87 1.716 4.95 )
					Azimuth ( 0.0 -5.0 5.0 )
					Transition ( 0 )
					Radius ( 0.5 )
					)
				)
			)
		Light	(
			comment( Head light left dim )
			Type( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 2 )
				)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle	( 0 )
			States	( 1
				State	(
					Duration ( 0.0 )
					LightColour ( cdffffd5 )
					Position ( 0.87 1.716 4.95 )
					Azimuth ( 0.0 -5.0 5.0 )
					Transition ( 0 )
					Radius ( 0.5 )
					)
				)
			)
		)

	Sound ( "380Eng.sms" )
)

Engine ( FS_GR740_084   
	Effects
	(
		SteamSpecialEffects
		(
			comment
			(
				the format of these little blocks is as follow:

				offset.x offset.y offset.z
				normal.x normal.y normal.z
				width in metres

				defining the offset from the shape pivot point
				where steam / smoke should appear, the direction
				it should go and the width of the nozzle
			)

			WhistleFX
			(
				-0.704 4.096 -3.492
				0 1 1
				0.2
			)

			SafetyValvesFX
			(
				0 3.885 -4.062
				0 1 0
				0.2

			)

			StackFX
			(
				0 4.3 3.75
				0 1.25 0
				0.35
			)

			DrainpipeFX
			(
				-1.5 1.258 -3.886
				-0.4 -1 -0.2
				0.05
			)

			CylindersFX
			(
				-0.357 0.8775 3.12
				-0.15 -.25 -.3
				0.025
			)

			CylindersFX
			(
				0.357 0.8775 3.12
				0.15 -.25 -0.3
				0.025
			)
		)
	)

	Wagon ( FS_GR740_084 )
	Type ( Steam )
	MaxPower ( 980hp )
	MaxForce ( 29400lbf )
	MaxVelocity ( 40mph )
	IsTenderRequired( 1 )
	WheelRadius ( 0.685m )
	Sanding ( 1e9mph )
	NumWheels ( 8 )
	BoilerLength ( 3.124m )
	BoilerVolume ( "22*(ft^3)" )
	BoilerEffectivity ( 1.00 )
	DraftingEffect ( 0.8 )
	BoilerResponsiveness ( 1.22 )
	CoalBurnage ( 3.6lb/hp/h )
	MaxBoilerOutput ( 32500lb/h )
	NumCylinders ( 2 )
	CylinderStroke ( 24in )
	CylinderDiameter ( 17.5in )
	CylinderVolume ( "3.8*(ft^3)" )
	CylinderEffectivity ( 1 )
	InjectorSizes ( 11mm 12mm )
	ExhaustLimit ( 33000lb/h )
	PrimingFactor ( 1 )
	BlastExponent ( 0.95 )
	MaxBoilerPressure ( 200psi )
	MaxFireMass ( 2500lb )
	IdealFireMass ( 1800lb )
	MaxWaterMass ( 4200lb )
	SafetyValvesSteamUsage ( 8000lb/h )
	ShovelCoalMass ( 1lb )
	SmokeCombustion ( 1 )
	SteamSmokeUnitsPerPoundOfFuel( 5.5 )
	MaxTenderCoalMass ( 7275lb )
	MaxTenderWaterMass ( 10000lb )
	comment( 0 for live steam, 1 for exhaust steam )
	InjectorTypes( 0 1 )
	SuperHeater ( 1.15 )
	SteamFiremanMaxPossibleFiringRate( 7000 )
	SteamGaugeGlassHeight( 11 )
	
	MaxSteamHeatingPressure( 80 )
	SafetyValvePressureDifference( 5 )

	BasicSteamUsage ( 1000lb/h )
	BasicCoalUsage ( 850lb/h )
	InjectorLimits1 ( 50psi 0.6 1 )  
	InjectorLimits2 ( 60psi 0.5 1 )  
	CylinderCocksPowerEfficiency ( 0.9 )
	
	TrainBrakesControllerMaxReleaseRate( 10 )
	TrainBrakesControllerMaxApplicationRate( 10 )
	TrainBrakesControllerEmergencyApplicationRate( 35 )
	TrainBrakesControllerMinSystemPressure( 0 )
	TrainBrakesControllerMaxSystemPressure( 70 )

	EngineBrakesControllerHasProportionalBrake( 1 )
        EngineBrakesProportionalBrakeLag( 0.9 )
        
        TrainBrakesControllerMaxPressureDropInNormalApplication( 70 )

	BrakesEngineBrakeType( "Air_single_pipe"  )
	BrakesTrainBrakeType( "Air_single_pipe" )
        BrakesEngineControllers( "Hand, Train, Independent" )

	SteamCylinderCocksOperation( Manual )
	SteamSmallestCutoff( 0.08 )
	NumberOfDamperSteps( 4 )

	RegulatorValveType( Twin_port )
	RegulatorSecondValveStartPosition( 0.45 )
	RegulatorPilotValveExponent( 1.7 )
	RegulatorSecondValveExponent( 1.7 )
	RegulatorPilotValveFullOpenning( 0.35 )
	RegulatorMainValveInitialOpenning( 0.475 )

	SteamBlowerEffectExponent( 0.9 )
	SteamBlowerEfficiencyExponent( 1.1 )
	comment( lbs/h )
	SteamBlowerMaxSteamUsageRate( 500 )
	SteamBlowerMaxProportionOfBlastEffect( 0.15 )

    	AirBrakesAirCompressorPowerRating( 3 )
    	AirBrakesMainMinResAirPressure( 0 )
    	AirBrakesMainMaxAirPressure( 100 )
	AirBrakesMainResVolume( 8 )
    	AirBrakesCompressorRestartPressure( 95 )
	AirBrakesAirUsedPerPoundsOfBrakePipePressure( 0.25 )

    	EngineBrakesControllerHasProportionalBrake( 1 )

	TrainBrakesControllerMaxApplicationRate( 5 )
	TrainBrakesControllerMaxReleaseRate( 10 )
	TrainBrakesControllerEmergencyApplicationRate( 10 )
	TrainBrakesControllerMinSystemPressure( 0 )
	TrainBrakesControllerMaxSystemPressure( 70 )

	EngineBrakesControllerMaxApplicationRate( 6 )
	EngineBrakesControllerMaxReleaseRate( 6 )
	EngineBrakesControllerMinSystemPressure( 0 )
	EngineBrakesControllerMaxSystemPressure( 70 )

	CabView ( 380.cvf )
	
	HeadOut ( -1.7 3.1 -5.5 )

        EngineControllers (
            Regulator ( 0 1 0.025 0 
                NumNotches( 0 )
            )
            Cutoff    ( -0.89 0.89 0.01 0 
                NumNotches( 0 )
            )
            Brake_Engine ( 0 1 0.0125 0
                NumNotches( 3
                    Notch(0    1 EngineBrakesControllerReleaseStart )
                    Notch(0.45 1 EngineBrakesControllerHoldStart )
                    Notch(0.5  1 EngineBrakesControllerApplyStart )
                )
            )            
            Brake_Train ( 0 1 0.0125 0.6 
                NumNotches( 4
                    Notch(0    1 TrainBrakesControllerReleaseStart )
                    Notch(0.4  1 TrainBrakesControllerSelfLapStart )
                    Notch(0.5  1 TrainBrakesControllerApplyStart )
                    Notch(0.9  1 TrainBrakesControllerEmergencyStart )
                )
            )
            Brake_Hand ( 0 1 0.0125 0 
                NumNotches( 0 )
            )
            FireDoor ( 0 1 0.1 0 
                NumNotches( 0 )
            )
            Sanding( 0 1 0 )
            Blower ( 0 1 0.025 0.2 
                NumNotches( 0 )
            )
            HeatingTap ( 0 1 0.1 0 
                NumNotches( 0 )
            )
            Shovel ( 0 1 0.1 0 
                NumNotches( 0 )
            )
            DampersFront ( 0 1 0.1 1
                NumNotches( 0 )
            )
            DampersBack ( 0 1 0.1 0 
                NumNotches( 0 )
            )
            Injector1Steam ( 0 1 0 )
            Injector2Steam ( 0 1 0 )
            Injector1Water ( 0 1 0.1 0 
                NumNotches( 0 )
            )
            Injector2Water ( 0 1 0.1 0 
                NumNotches( 0 )
            )
            CylinderCocks ( 0 1 1 )
            Whistle ( 0 1 0 )
            SmallEjectorOrCompressor( 0 1 1 )
            BellToggle( 0 1 0 )
            Headlights( 0 1 0 )
        )
	comment(fire temp, fire mass, water mass, boiler pressure,
		tender_water_mass, tender_coal_mass,
		smoke_quantity, fire_condition, coal quality )
	EngineVariables( 770 2650 3750 200 50000 18000 350 1 1 )
	Sound ( "380Cab.sms" )
	Name ( "FS Gr. 740.084" )
	Description (
	"Locomotiva a vapore per treni merci."
	)
	EngineOperatingProcedures (
	"To move forward\n"+
	"1.	Press the W key several times to move the Reverser to full Forward.\n"+
	"2.	Press the ; (SEMICOLON) key to release the train brakes.\n"+
	"3.	Press the [ (LEFT BRACKET) key to release the locomotive brake.\n"+
	"4.	Press the D key to increase the Regulator setting.\n"+  
	"5.	As you accelerate, press the S key to slowly reduce the Reverser setting, then adjust the Regulator to maintain the desired speed.\n\n"+ 
	"To slow the train\n"+
	"1.	Press the A key to move the Regulator to a lower setting.\n"+
	"2.	Use the brakes to further reduce speed if desired.\n\n"+   
	"To apply the train brakes\n"+
	"1.	Press the ' (APOSTROPHE) key to apply the train brakes.\n\n"+
	"To release the train brakes\n"+
	"1. Press the ; (SEMICOLON) key to release the train brakes.\n\n"+
	"To apply the locomotive brake\n"+
	"1.	Press the ] (RIGHT BRACKET) key to apply the locomotive brake.\n\n"+
	"To release the locomotive brake\n"+
	"1. Press the [ (LEFT BRACKET) key to release the locomotive brake.\n\n"+
	"To back up\n"+
	"1.	Bring your train to a full stop.\n"+
	"2.	Press the S key several times to move the Reverser to the full Reverse position.\n"+
	"3.	Press the ; (SEMICOLON) key to release the brakes.\n"+
	"4.	Slowly advance the Regulator (D key).\n\n"+
	"To load and unload passengers\n"+
	"1. Stop at a station.\n"+
	"2. Press the ENTER key.\n"+
	"3. Wait for the \"permission to depart\" whistle.\n"+
	"TIP: Use the Next Station driving aid (F10) to monitor loading and unloading.\n\n"+
	"To couple to a car or locomotive\n"+
	"1. Coast into the unit at a very slow speed, about 4 Km/h.\n"+
	"TIP: To use the Coupling view, press the 6 key.\n"+
	"2. Press F9 to open the Train Operations window.\n"+
	"3. If the icon for the unit you coupled to is red, the handbrake is on. Double-click the car to release the handbrake.\n"+
	"4. Close the Train Operations window.\n\n"+
	"To uncouple from a car or locomotive\n"+
	"1. Press F9 to open the Train Operations window.\n"+
	"2. Double-click a unit in the part of the train you want to uncouple from the locomotive, to set the handbrake.\n"+
	"3. Double-click the coupler between the units you want to uncouple and the rest of the train.\n"+
	"4. Click the green 'coupler' between the units you want to uncouple.\n"+
	"5. Click the Uncouple button.\n"+
	"6. Close the Train Operations window.\n\n"+
	"Firing commands (Automatic Fireman OFF in Options screen)\n"+
	"To add coal to the firebox\n"+
	"1. Press the F key to open the Firebox door.\n"+
	"2. Press the R key to increase the shoveling rate.\n\n"+
	"To stop adding coal to the fire\n"+
	"1. Press SHIFT+R to decrease the shoveling rate.\n"+
	"2. Press SHIFT+F to close the firebox door.\n"+
	"To operate the blower\n\n"+
	"1.	Press the N key to increase the blower.\n"+
	"2. Press SHIFT+N to decrease the blower.\n\n"+
	"To operate the dampers\n"+
	"1.	Press the M key to open the dampers.\n"+
	"2. Press SHIFT+M to close the dampers.\n\n"+
	"To inject water into the boiler\n"+
	"1.	Press the I key to turn on the steam to Injector 1.\n"+
	"(You can also press the O key to turn on the steam to Injector 2.)\n"+
	"2.	Press the K key to increase the water flow to Injector 1.\n"+
	"(To increase the water flow to Injector 2, press the L key.)\n\n"+
	"To stop boiler water injection\n"+
	"1. Press the I key to turn off the steam to Injector 1.\n"+
	"2. Press the O key to turn off the steam to Injector 2."
	)
)
