SIMISA@@@@@@@@@@JINX0D0t______

Wagon ( FS_Gr270_089  
	Type ( Engine )
	WagonShape ( FS_Gr270_089.s )
	Size  ( 2.7m 4.12m 9.00m )
	CentreOfGravity ( 0m 1.86m 0m )
	Centre ( 0m 0m 0m )
	Mass ( 43.60t # aderenti 43.6t )
	InertiaTensor ( Box(2.7m 4.0m 9.00m) )
	Coupling (
		Type ( Bar )
		Spring (
			Stiffness ( 1e7N/m 1e6N/m )
			Damping ( 2e6N/m 2e6N/m)
			r0 ( 10cm 20cm )
		)
	)
	Coupling (
		Type ( Chain )
		Spring (
			Stiffness ( 1e7N/m 1e6N/m )
			Damping ( 2e6N/m 2e6N/m)
			r0 ( 10cm 20cm )
		)
	)
	
	Buffers (
		Spring (
			Stiffness ( 1e6N/m 5e6N/m )
			Damping ( 1e6N/m/s 1e6N/m/s )
			r0 ( 0m 1e9 )
		)
		Centre ( 0.5 )
		Radius ( 1 )
		Angle ( 0.5deg )
	)

	Adheasion ( 0.1725 0.345 3.00 0.5 )
	DerailRailHeight ( 4cm )
	DerailRailForce ( 109kN )
	DerailBufferForce ( 174.4kN )
	WheelRadius ( 0.92m )
	NumWheels ( 6 )
	Friction (
		2982N/m/s			0		1mph		12.11N/m/s		1.8
		5.1N/rad/s		1		-1rad/s		0		1
	)

	BrakeEquipmentType( "Triple_valve, Auxilary_reservoir, Handbrake " )
	BrakeSystemType( "Air_single_pipe" )
	MaxBrakeForce( 43.6kN )

	MaxHandbrakeForce( 30kN )
	NumberOfHandbrakeLeverSteps( 100 )

	TripleValveRatio( 2.5 )
	MaxReleaseRate( 15 )
	MaxApplicationRate( 15 )
	MaxAuxilaryChargingRate( 15 )
      BrakeCylinderPressureForMaxBrakeBrakeForce( 70 )


	Lights	( 5
		Light	(
			comment( Sphere of light )
			Type( 1 )
			Conditions(
				Headlight ( 3 )
				Unit ( 2 )
				)
			Cycle	( 0 )
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			States	( 1
				State	(
					Duration ( 0.0 )
					LightColour ( ffffffd5 )
					Position ( 0.0 10 0 )
					Transition ( 0 )
					Radius ( 160.0 )
					Angle ( 25.0 )
					)
				)
			)
			
		
		Light	(	
			comment( Head light right dim )
			Type( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 2 )
				)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle	( 0 )
			States	( 1
				State	(
					Duration ( 0.0 )
					LightColour ( cdffffd5 )
					Position ( -0.852 1.49 3.98 )
					Azimuth ( 0.0 0.0 5.0 )
					Transition ( 0 )
					Radius ( 0.5 )
					)
				)
			)
		Light	(	
			comment( Head light right dim )
			Type( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 2 )
				)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle	( 0 )
			States	( 1
				State	(
					Duration ( 0.0 )
					LightColour ( cdffffd5 )
					Position ( -0.852 1.49 3.98 )
					Azimuth ( 0.0 0.0 5.0 )
					Transition ( 0 )
					Radius ( 0.5 )
					)
				)
			)

		Light	(
			comment( Head light left dim )
			Type( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 2 )
				)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle	( 0 )
			States	( 1
				State	(
					Duration ( 0.0 )
					LightColour ( cdffffd5 )
					Position ( 0.852 1.49 3.98 )
					Azimuth ( 0.0 -5.0 5.0 )
					Transition ( 0 )
					Radius ( 0.5 )
					)
				)
			)
		Light	(
			comment( Head light left dim )
			Type( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 2 )
				)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle	( 0 )
			States	( 1
				State	(
					Duration ( 0.0 )
					LightColour ( cdffffd5 )
					Position ( 0.852 1.490 3.98 )
					Azimuth ( 0.0 -5.0 5.0 )
					Transition ( 0 )
					Radius ( 0.5 )
					)
				)
			)
		)
	Sound ( "..\\..\\common.sound\\2cyl_generic\\2c-100b-eng01.sms" )
)

Engine ( FS_Gr270_089   
	Effects
	(
		SteamSpecialEffects
		(
			comment
			(
				the format of these little blocks is as follow:

				offset.x offset.y offset.z
				normal.x normal.y normal.z
				width in metres

				defining the offset from the shape pivot point
				where steam / smoke should appear, the direction
				it should go and the width of the nozzle
			)

			WhistleFX
			(
				0 4.124 -3.009
				0 1 1
				0.2
			)

			SafetyValvesFX
			(
				0 3.5 -2.3
				0 1 0
				0.2

			)

			StackFX
			(
				0 4.2 2.93
				0 1.25 0
				0.35
			)

			DrainpipeFX
			(
				-1.5 1.258 -3.886
				-0.4 -1 -0.2
				0.05
			)

			CylindersFX
			(
				-0.357 0.975 3.12
				-1 0 0
				0.1
			)

			CylindersFX
			(
				0.357 0.975 3.12
				1 0 0
				0.1
			)
		)
	)

	Wagon ( FS_Gr270_089 )
      Type ( Steam )
	IsTenderRequired( 1 )

Comment ( Valori Massimi Dinamica )

	MaxPower ( 323.84kw )
	MaxForce ( 73.5kn )
	MaxVelocity ( 37.5mph )
	
Comment ( Parametri Ruote )

	WheelRadius ( 0.755m )
	Sanding ( 20mph )
	NumWheels ( 6 )

Comment ( Caldaia )

	BoilerLength ( 3.6m )
	BoilerVolume ( "215.46*(ft^3)" )
	BoilerEffectivity ( 1.00 )
	DraftingEffect ( 0.85 )
	BoilerResponsiveness ( 1.2 )
	MaxBoilerOutput ( 15162.35lb/h )
	MaxBoilerPressure ( 170.70psi )
	MaxWaterMass ( 9368lb )

Comment ( Forno )

	CoalBurnage ( 4lb/hp/h )
	MaxFireMass ( 1440lb )
	IdealFireMass ( 1080lb )

Comment ( Surriscaldamento )

      SuperHeater ( 1.0 ) comment ( vapore surriscaldato )
	MaxSteamHeatingPressure( 80 ) comment ( idem )  

Comment ( Cilindri )
	
	NumCylinders ( 2 )
	CylinderStroke ( 65cm )
	CylinderDiameter ( 25.5cm )
	CylinderVolume ( "6.98*(ft^3)" )
	CylinderEffectivity ( 1.2 )

Comment ( Iniettori )

	InjectorSizes ( 12mm 12mm )
	InjectorTypes( 0 1 )
	
	
Comment ( Valvole Sicurezza )
	
	SafetyValvesSteamUsage ( 10000lb/h )
	SafetyValvePressureDifference( 3 )

Comment ( Fuochista )

	ShovelCoalMass ( 1lb )
	SteamFiremanMaxPossibleFiringRate( 4414 )
	SteamMaxSmokeUnitsReleaseRate( 0.5 )

Comment ( Fumo )

	SmokeCombustion ( 1 )
	SteamSmokeUnitsPerPoundOfFuel( 5.5 )

Comment ( Tender )

	MaxTenderCoalMass ( 7040lb ) 
	MaxTenderWaterMass ( 17600lb )

Comment ( Altri Parametri )

	ExhaustLimit ( 15466lb/h )
	PrimingFactor ( 1 )
	BlastExponent ( 1 )
	SteamGaugeGlassHeight( 6.9 )

Comment ( Consumi - Limiti Efficienza )

	BasicSteamUsage ( 3790.59lb/h )
	BasicCoalUsage ( 1895.29lb/h )
	InjectorLimits1 ( 50psi 0.6 1 )  
	InjectorLimits2 ( 60psi 0 1 )  
	CylinderCocksPowerEfficiency ( 0.85 )

	SteamCylinderCocksOperation( manual )
	SteamSmallestCutoff( 0.08 )
	NumberOfDamperSteps( 4 )

	RegulatorValveType( Twin_port )
	RegulatorSecondValveStartPosition( 0.23 )
	RegulatorPilotValveExponent( 1.7 )
	RegulatorSecondValveExponent( 1.7 )
	RegulatorPilotValveFullOpenning( 0.49 )
	RegulatorMainValveInitialOpenning( 0.495 )

      SteamBlowerEffectExponent( 0.6 )
	SteamBlowerEfficiencyExponent( 1 )
	SteamBlowerMaxSteamUsageRate( 500 )	comment( lbs/h )
	SteamBlowerMaxProportionOfBlastEffect( 0.255 )

	BrakesEngineBrakeType( "Air_single_pipe"  )
	BrakesTrainBrakeType( "Air_single_pipe" )
      BrakesEngineControllers( "Hand, Train, Independent" )

    	AirBrakesAirCompressorPowerRating( 3 )
    	AirBrakesMainMinResAirPressure( 0 )
    	AirBrakesMainMaxAirPressure( 100 )
	AirBrakesMainResVolume( 40 )
    	AirBrakesCompressorRestartPressure( 65 )
	AirBrakesAirUsedPerPoundsOfBrakePipePressure( 3 )	
	AirBrakesHasLowPressureTest(1) 
	AirBrakesIsCompressorElectricOrMechanical(1)

      TrainBrakesControllerMaxPressureDropInNormalApplication( 70 )
	TrainBrakesControllerMaxReleaseRate( 4 )
	TrainBrakesControllerMaxApplicationRate ( 5 )
	TrainBrakesControllerMinSystemPressure( 0 )
	TrainBrakesControllerMaxSystemPressure( 72 ) 
	TrainPipeLeakRate (0.9 )

	EngineBrakesControllerHasProportionalBrake( 1 )
      EngineBrakesProportionalBrakeLag( 1 )
	EngineBrakesControllerMaxApplicationRate( 5 )
	EngineBrakesControllerMaxReleaseRate( 5 )
	EngineBrakesControllerMinSystemPressure( 0 )
	EngineBrakesControllerMaxSystemPressure( 100 )

	CabView ( 380.cvf )
	
	HeadOut ( -1.595 3.162 -5.246 )

        EngineControllers (
            Regulator ( 0 1 0.02 0 
                NumNotches( 0 )
            )
            Cutoff    ( -0.89 0.89 0.01 0.415 
                NumNotches( 0 )
            )
            Brake_Engine ( 0 1 0.0125 0
                NumNotches( 3
                    Notch(0    1 EngineBrakesControllerReleaseStart )
                    Notch(0.45 1 EngineBrakesControllerHoldStart )
                    Notch(0.5  1 EngineBrakesControllerApplyStart )
                )
            )            
            Brake_Train ( 0 1 0.02 0.4
                NumNotches( 5
                    Notch(0    0 TrainBrakesControllerReleaseStart )
                    Notch(0.1  0 TrainBrakesControllerNeutralHandleOffStart )
                    Notch(0.2  1 TrainBrakesControllerApplyStart )
                    Notch(0.9  0 TrainBrakesControllerFullServiceStart )
                    Notch(0.99  0 TrainBrakesControllerEmergencyStart )
                )
            )
            Brake_Hand ( 0 1 0.0125 0 
                NumNotches( 0 )
            )
            FireDoor ( 0 1 0.1 0 
                NumNotches( 0 )
            )
            Sanding( 0 1 0 )
            Blower ( 0 1 0.025 0.2 
                NumNotches( 0 )
            )
            HeatingTap ( 0 1 0.1 0 
                NumNotches( 0 )
            )
            Shovel ( 0 1 0.1 0 
                NumNotches( 0 )
            )
            DampersFront ( 0 1 0.1 1
                NumNotches( 0 )
            )
            DampersBack ( 0 1 0.1 0 
                NumNotches( 0 )
            )
            Injector1Steam ( 0 1 0 )
            Injector2Steam ( 0 1 0 )
            Injector1Water ( 0 1 0.1 0 
                NumNotches( 0 )
            )
            Injector2Water ( 0 1 0.1 0 
                NumNotches( 0 )
            )
            CylinderCocks ( 0 1 1 )
            Whistle ( 0 1 0 )
            SmallEjectorOrCompressor( 0 1 1 )
            BellToggle( 0 1 0 )
            Headlights( 0 1 0 )
        )
	comment(fire temp, fire mass, water mass, boiler pressure,
		tender_water_mass, tender_coal_mass,
		smoke_quantity, fire_condition, coal quality )

	EngineVariables( 770 1188 7213.3 170.87 0.77 17600 7040 350 1 1 )
	Sound ( "..\\..\\common.sound\\2cyl_generic\\2c-100b-cab01.sms" )

	Name ( "FS Gr 270.089" )
	Description (
	"Locomotiva a vapore per servizio passeggeri veloce\n"+
	"Costruite in 130 esemplari tra il 1888 ed il 1891\n"+
	"Dati della locomotiva reale:\n"+
	"Velocità massima: 60 km/h \n"+
	"Potenza: 440 CV a 30 km/h \n"+
	"Pressione caldaia: 12 kg/cm²\n"+
	"Massa in servizio: 43.60 t \n"+
	"Massa aderente: 43.60 t \n"+
	"Rodiggio: 0-3-0 \n"+
	"Cilindri:  2 esterni \n"+
	"Distribuzione: Stephenson "

	)
	EngineOperatingProcedures (
	"To move forward\n"+
	"1.	Press the W key several times to move the Reverser to full Forward.\n"+
	"2.	Press the ; (SEMICOLON) key to release the train brakes.\n"+
	"3.	Press the [ (LEFT BRACKET) key to release the locomotive brake.\n"+
	"4.	Press the D key to increase the Regulator setting.\n"+  
	"5.	As you accelerate, press the S key to slowly reduce the Reverser setting, then adjust the Regulator to maintain the desired speed.\n\n"+ 
	"To slow the train\n"+
	"1.	Press the A key to move the Regulator to a lower setting.\n"+
	"2.	Use the brakes to further reduce speed if desired.\n\n"+   
	"To apply the train brakes\n"+
	"1.	Press the ' (APOSTROPHE) key to apply the train brakes.\n\n"+
	"To release the train brakes\n"+
	"1. Press the ; (SEMICOLON) key to release the train brakes.\n\n"+
	"To apply the locomotive brake\n"+
	"1.	Press the ] (RIGHT BRACKET) key to apply the locomotive brake.\n\n"+
	"To release the locomotive brake\n"+
	"1. Press the [ (LEFT BRACKET) key to release the locomotive brake.\n\n"+
	"To back up\n"+
	"1.	Bring your train to a full stop.\n"+
	"2.	Press the S key several times to move the Reverser to the full Reverse position.\n"+
	"3.	Press the ; (SEMICOLON) key to release the brakes.\n"+
	"4.	Slowly advance the Regulator (D key).\n\n"+
	"To load and unload passengers\n"+
	"1. Stop at a station.\n"+
	"2. Press the ENTER key.\n"+
	"3. Wait for the \"permission to depart\" whistle.\n"+
	"TIP: Use the Next Station driving aid (F10) to monitor loading and unloading.\n\n"+
	"To couple to a car or locomotive\n"+
	"1. Coast into the unit at a very slow speed, about 4 Km/h.\n"+
	"TIP: To use the Coupling view, press the 6 key.\n"+
	"2. Press F9 to open the Train Operations window.\n"+
	"3. If the icon for the unit you coupled to is red, the handbrake is on. Double-click the car to release the handbrake.\n"+
	"4. Close the Train Operations window.\n\n"+
	"To uncouple from a car or locomotive\n"+
	"1. Press F9 to open the Train Operations window.\n"+
	"2. Double-click a unit in the part of the train you want to uncouple from the locomotive, to set the handbrake.\n"+
	"3. Double-click the coupler between the units you want to uncouple and the rest of the train.\n"+
	"4. Click the green 'coupler' between the units you want to uncouple.\n"+
	"5. Click the Uncouple button.\n"+
	"6. Close the Train Operations window.\n\n"+
	"Firing commands (Automatic Fireman OFF in Options screen)\n"+
	"To add coal to the firebox\n"+
	"1. Press the F key to open the Firebox door.\n"+
	"2. Press the R key to increase the shoveling rate.\n\n"+
	"To stop adding coal to the fire\n"+
	"1. Press SHIFT+R to decrease the shoveling rate.\n"+
	"2. Press SHIFT+F to close the firebox door.\n"+
	"To operate the blower\n\n"+
	"1.	Press the N key to increase the blower.\n"+
	"2. Press SHIFT+N to decrease the blower.\n\n"+
	"To operate the dampers\n"+
	"1.	Press the M key to open the dampers.\n"+
	"2. Press SHIFT+M to close the dampers.\n\n"+
	"To inject water into the boiler\n"+
	"1.	Press the I key to turn on the steam to Injector 1.\n"+
	"(You can also press the O key to turn on the steam to Injector 2.)\n"+
	"2.	Press the K key to increase the water flow to Injector 1.\n"+
	"(To increase the water flow to Injector 2, press the L key.)\n\n"+
	"To stop boiler water injection\n"+
	"1. Press the I key to turn off the steam to Injector 1.\n"+
	"2. Press the O key to turn off the steam to Injector 2."
	)
)
