This upgrade patch will only work with Route_Riter v6.2.55
or later which will be upgraded to v6.2.75

INSTALLATION
------------
1. Unzip this archive into a temporary folder and READ this file.

2. DELETE THE FOLDER TSUTIL from your existing Route_Riter folder.

3. Copy the new TSUTIL folder and the file Route_Riter.exe into your
existing Route_Riter folder.

RECENT ADDITIONS TO ROUTE-RITER
-------------------------------
v6.2.73 includes a new option to Activate/Deactivate Routes in MSTS.
This works similarly to the program 'Routes on/off' but works on systems
with multiple installations of MSTS. Deactivating a route simply renames
the route's .trk file (e.g. Europe1.trk to Europe1.off). Reactivating it
turns the route back on. This makes MSTS load much faster. Using this option
will also show which routes are on/off, and for users of Train-Store this
will indicate which are probably in store (but will not unstore them
for you).

Also included is an option to Fix .CVF Files, first run Conbuilder to
Test Locomotive files with the CabView box ticked. This will tell you how
many faulty CabView entries there are. Then run RR and click the Fix .CVF
files button. Once this completes, try Conbuilder again and see the difference
In my case this dropped from 214 to 18.

There is also an option on the Edit Unicode screen to automatically alias
Sound and Cabviews - Suggest you download the latest RR help file for further
details.

New to this version are:-
a) Activities/Stock - new button 'List Stock for Selected Consists' 
Self explanatory, select consist(s) and click this button and you will
get a list of all the stock required for the consists selected. (Click the
remove duplicates button so that just one of each item is listed). List
may be printed or saved.
b) MSTS file Utils - The Zero Error Bias has been altered to 'Normalise
.T ErrorBias' - This button changes the Terrain Error Bias entries in the selected
route to the value you enter in the Box. The value in the .trk file is now changed
as well, I missed this in the earlier version.

Please see http://members.optusnet.com.au/virtualtrains/faq.html
for common queries.

Please advise of any problems.

Those of you who did not get v6.2.64 will have missed the following instructions
for setting up Hard-Links 
quote
Route-Riter - Setting up Common Shapes/Textures for MSTS
--------------------------------------------------------

The 'Holy-Grail' of MSTS users has always been to have a 'Global Folder'
for Shapes and Textures. Up to now, this has always been considered
virtually impossible to achieve.

However following some work done by 'Mdanie' on uktrainsim.com and
suggestions from other users, it has been discovered that at least for
users who use Windows XP with the NTFS file system that this is possible.

XP includes a command 'Fsutil Hardlink Create file-A file-B' this in effect 
places a directory link for file-A pointing to the position of file-B on the 
hard-drive. Deleting either A or B has no effect on the other, the file
is only removed from the drive when both A and B are deleted. These files
appear in Windows Explorer with exactly the same entries as before, so folder
size etc remains the same. The difference is in the free space on the drive.

In my case, I had two versions of the London South-East route on my E: drive 
one in my main MSTS installation, one as a mini-route. The saving by using 
a common folder was 740 mb for a single route.

In RR v6.2.64, I have implemented this to some extent using a new tab 'Link 
Shapes/Textures' - The procedure is as follows:-

a) Set up a Common Folder (use the button 'Set up Common Files' under Misc
Options) - You may if you wish then click the Copy Default Files to Common 
so that all the default files are now in the common folder.
Note: The Common folder MUST be on the same hard-drive as your MSTS folder, 
usually in your Routes folder. The hard-drive MUST run under XP with the NFTS
file system.
b) Select the Common folder from the Files menu (once you do this once, it
is saved for future use and should not need to be selected again).
c) For any route you wish to use this option with, you should now copy the 
Shapes/Textures/Terrtex/Envfiles/Sound folders into the Common folder (use
the 'Copy Route Files to Common Folder' button).
d) Select the Route as usual by clicking the Confirm Route button
e) Click the 'Link all Files to Common Files' button and the hard links are set up.
f) Check your hard-drive free space before/after.

Note: In some cases, files in the Common folder might have the same name but 
be different to the one used by a particular route. A crc check is made, and
if different, then the file is not replaced by a hardlink.

The above is somewhat experimental, so I would only suggest experimenting
with routes which you have backups for in the early stages.

In v6.2.64, I have added two further buttons:-

a. 'List Hard Links in Common Files' shows you a list of all the files in the
Common files folder and how many links each file has. A reading of '1' link
means that the file is not linked to any route, so may be removed to reduce space
There is a button on this screen which will delete all unlinked files.

b. 'List Linked Files in Selected Route' shows which files in the route
are linked (once again, those showing 1 link are unlinked - the single link
is the link from the file name to the file on the hard-drive).
unquote

Mike Simpson - 13th Jul 2005
virtualtrains@optushome.com.au
http://members.optusnet.com.au/virtualtrains

