	Comment ( Use on all 4 axle and small six-axle diesel engines up to SD24 and GE U-Boat in size )
	Comment ( All larger Road units should use the Large Engine Coupler )
	Coupling (
		Type ( Automatic )
		Spring (
			Stiffness ( 2e3N/m 4.5e6N/m )
			Damping ( 1e6N/m/s 1e6N/m/s )
			Break ( 5.1e7N 5.1e7N )
			r0 ( 10cm 15cm )
		)
		Velocity ( 0.2m/s )
	)
	Coupling (
		Type ( Automatic )
		Spring (
			Stiffness ( 2e3N/m 4.5e6N/m )
			Damping ( 1e6N/m/s 1e6N/m/s )
			Break ( 5.1e7N 5.1e7N )
			r0 ( 10cm 15cm )
		)
		Velocity ( -0.2m/s )
	)
	Buffers (
		Spring (
			Stiffness ( 1e6N/m 5e6N/m )
			Damping ( 1e6N/m/s 1e6N/m/s )
			r0 ( 0m 1e9 )
		)
		Centre ( 0.5 )
		Radius ( 1 )
		Angle ( 0.5deg )
	)