	comment ( For cars equiped with cushioned drawbar type couplers ie: Centerbeam flats, bulkhead flats ) 
	comment ( newer boxcars, newer flats, cabooses, and other common cars were freight durability is an )
	comment ( issue. Note: Use MSTS Bin Long Cushioned coupler for Autoracks )
	Coupling (
		Type ( Automatic )
		Spring (
			Stiffness ( 8e2N/m 4.5e6N/m )
			Damping ( 2e6N/m/s 2e6N/m/s )
			Break ( 5.1e7N 5.1e7N )
			r0 ( 12cm 12cm )
		)
		Comment ( CouplingHasRigidConnection ( 1 ) )
		Velocity ( 0.2m/s )
	)
	Coupling (
		Type ( Automatic )
		Spring (
			Stiffness ( 8e2N/m 4.5e6N/m )
			Damping ( 2e6N/m/s 2e6N/m/s )
			Break ( 5.1e7N 5.1e7N )
			r0 ( 12cm 12cm )
		)
		CouplingHasRigidConnection ( 1 )
		Velocity ( -0.2m/s )
	)
	Buffers (
		Spring (
			Stiffness ( 1e6N/m 5e6N/m )
			Damping ( 1e6N/m/s 1e6N/m/s )
			r0 ( 0m 1e9 )
		)
		Centre ( 0.5 )
		Radius ( 1 )
		Angle ( 0.5deg )
	)