	Comment ( For excessive length cars over 75ft equiped with cushioned drawbar couplers )
	Comment ( ie:  86foot Boxcars, autoracks, intermodal flatcars (TOFC only) and flatcars. )
	Comment ( Note:  Use regular cushioned drawbar couplers for Centerbeam and Bulkhead flatcars. )

	Coupling (
		Type ( Automatic )
		Spring (
			Stiffness ( 5e6N/m 5e6N/m )
			Damping ( 1e6N/m/s 4e6N/m/s )
			Break ( 5.1e7N 5.1e7N )
			r0 ( 30cm 30cm )
		)
		Comment ( CouplingHasRigidConnection ( 1 ) )
		Velocity ( 0.2m/s )
	)
	Coupling (
		Type ( Automatic )
		Spring (
			Stiffness ( 5e6N/m 5e6N/m )
			Damping ( 1e6N/m/s 4e6N/m/s )
			Break ( 5.1e7N 5.1e7N )
			r0 ( 30cm 30cm )
		)
		CouplingHasRigidConnection ( 1 )
		Velocity ( -0.2m/s )
	)
	Buffers (
		Spring (
			Stiffness ( 1e6N/m 5e6N/m )
			Damping ( 1e6N/m/s 5e6N/m/s )
			r0 ( 0m 1e9 )
		)
		Centre ( 0.5 )
		Radius ( 2 )
		Angle ( 10.5deg )
	)