	Comment ( Use on cars with Rigid couplers ie: Hopper cars, gondolas, tankcars, older flatcars and boxcars )
	  Coupling (
		Type ( Automatic )
		Spring (
			Stiffness ( 2e1N/m 5e6N/m )
			Damping ( 2e6N/m/s 2e6N/m/s )
			Break ( 5.1e7N 5.1e7N )
			r0 ( 5cm 8cm )
		)
		Comment ( CouplingHasRigidConnection ( 1 ) )
		Velocity ( 0.2m/s )
	  )
	  Coupling (
		Type ( Automatic )
		Spring (
			Stiffness ( 2e1N/m 5e6N/m )
			Damping ( 2e6N/m/s 2e6N/m/s )
			Break ( 5.1e7N 5.1e7N )
			r0 ( 5cm 8cm )
		)
		CouplingHasRigidConnection ( 1 )
		Velocity ( -0.2m/s )
 	  )
	  Buffers (
		Spring (
			Stiffness ( 5e6N/m 8e6N/m )
			Damping ( 1e6N/m/s 1e6N/m/s )
			r0 ( 0m 1e9 )
		)
		Centre ( 0.5 )
		Radius ( 1 )
		Angle ( 0.5deg )
 	  )